Highlights

1. Five basic connection types of Stirling engine array were summarized.
2. A new Stirling engine model was developed and validated.
3. Influence of flow type and flow order on the performance was investigated.
4. It was found that the flow order has little influence on the performance.